PCI audio DOS utilities instructions


* SETAUDIO.COM

DOS initial program

  The following are the parameters format:
/Gx : x=0 disable game port, x=1 enable (default)
/Mx : x=0 disable MPU-401 MIDI port, x=1 enable (default)
/IOxxx : Set SB I/O port to 220(default),240,260 or 280.
/FMxxx : Set FM I/O port to 388(default),3C8,3E0 or 3E8.
/MPUxxx : Set MPU-401 MIDI port to 330(default),320,310,300.


* FIXEPIC.EXE

EPIC DOS games patch program

  We found that there are some EPIC DOS games can not detect PCI 
audio. This is due to these games using instruction loop as time 
counter not a real constant period. In high speed CPU PC, the loop 
time become shorter. That is reason that games can not detect PCI 
audio. If you meet this problem, please run patch program to fix. 
All of fixed files will backup to *.old.